EXСLUSIVE FOR GTA.COM.UA TO 10.12.2012 (inclusive)!

                                                                                     AUTHORS
Arti9609
email: arti9609@yandex.ru



                                                                                 INSTALLATION

Install the model using Spark IV or Open IV, and standard "notepad".

-Open vehicles.img using Spark IV or Open IV
-Find model and replace the appropriate files from vehicles.img
-Find model necessary to you, press Import and choose the necessary files with expansion wdt and wft
-Replace the standard lines with the lines from readme.txt in appropriate files:
 [CARCOLS.DAT]

0,0,0,0, 1,27,102,27, 27,102,125,102, 128,24,83,24, 83,24,128,24, 133,27,113,27, 1,27,1,27, 120,1,120,1, 113,112,113,112, 127,127,127,127, 126,126,126,126, 112,113,112,113, 102,27,102,27, 20,27,21,20
 [VEHICLES.IDE]

blista,		blista,		car,		BLISTA,		BLISTA, VEH@STD, VEH@STD_LO4_LO4,  10, 999,  0.2724, 0.2724,  0, 5, 1.0 ,0, ext_gang+ext_all+ext_strong

[HANDLING.DAT]


1380.0 2.3 85 0.0 0.05 -0.83 1.0 5 0.15 1.0 197.0 0.22 0.63 0.5 32.0 1.37 1.6 10.0 0.13 0.465 2.5 1.8 1.6 0.11 -0.11 -0.009 0.505 1.0 1.0 1.0 1.0 0.0 42000 440010 0 1